From 2b88563ee5aafd9571d965b7f2093a0f58d98a31 Mon Sep 17 00:00:00 2001
From: John Crispin <john@phrozen.org>
Date: Thu, 26 Nov 2020 12:02:21 +0100
Subject: PHY: Increase max PHY adddress number

* rename the target to realtek
* add refactored DSA driver
* add latest gpio driver
* lots of arch cleanups
* new irq driver
* additional boards

Submitted-by: Bert Vermeulen <bert@biot.com>
Submitted-by: Birger Koblitz <mail@birger-koblitz.de>
Submitted-by: Sander Vanheule <sander@svanheule.net>
Submitted-by: Bjørn Mork <bjorn@mork.no>
Submitted-by: John Crispin <john@phrozen.org>
---
 include/linux/phy.h                           | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

--- a/include/linux/phy.h
+++ b/include/linux/phy.h
@@ -297,7 +297,7 @@ static inline const char *phy_modes(phy_
 #define PHY_INIT_TIMEOUT	100000
 #define PHY_FORCE_TIMEOUT	10
 
-#define PHY_MAX_ADDR	32
+#define PHY_MAX_ADDR	64
 
 /* Used when trying to connect to a specific phy (mii bus id:phy device id) */
 #define PHY_ID_FMT "%s:%02x"
