From 87363cc0e522de3294ea6ae10fb468d2a8d6fb2f Mon Sep 17 00:00:00 2001
From: OpenWrt community <openwrt-devel@lists.openwrt.org>
Date: Wed, 13 Jul 2022 12:17:21 +0200
Subject: [PATCH] spi-nor/esmt.c: add esmt f25l16pa

This fixes support for Dongwon T&I DW02-412H which uses F25L16PA(2S)
flash.

---
 drivers/mtd/spi-nor/esmt.c | 2 ++
 1 file changed, 2 insertions(+)

--- a/drivers/mtd/spi-nor/esmt.c
+++ b/drivers/mtd/spi-nor/esmt.c
@@ -10,6 +10,9 @@
 
 static const struct flash_info esmt_nor_parts[] = {
 	/* ESMT */
+	{ "f25l16pa-2s", INFO(0x8c2115, 0, 64 * 1024, 32)
+			FLAGS(SPI_NOR_HAS_LOCK)
+			NO_SFDP_FLAGS(SECT_4K) },
 	{ "f25l32pa", INFO(0x8c2016, 0, 64 * 1024, 64)
 		FLAGS(SPI_NOR_HAS_LOCK | SPI_NOR_SWP_IS_VOLATILE)
 		NO_SFDP_FLAGS(SECT_4K) },
