From 6cea7c46172eca323e9ce7e6aab8f8506eb92b4b Mon Sep 17 00:00:00 2001
From: Tim Harvey <tharvey@gateworks.com>
Date: Wed, 29 Nov 2023 09:53:04 -0800
Subject: [PATCH 405/413] 6.9: arm64: dts: imx8mm-venice-gw71xx: add TPM device

Add the TPM device found on the GW71xx revision E PCB.

Signed-off-by: Tim Harvey <tharvey@gateworks.com>
---
 .../arm64/boot/dts/freescale/imx8mm-venice-gw71xx.dtsi | 10 +++++++++-
 1 file changed, 9 insertions(+), 1 deletion(-)

--- a/arch/arm64/boot/dts/freescale/imx8mm-venice-gw71xx.dtsi
+++ b/arch/arm64/boot/dts/freescale/imx8mm-venice-gw71xx.dtsi
@@ -53,8 +53,15 @@
 &ecspi2 {
 	pinctrl-names = "default";
 	pinctrl-0 = <&pinctrl_spi2>;
-	cs-gpios = <&gpio5 13 GPIO_ACTIVE_LOW>;
+	cs-gpios = <&gpio5 13 GPIO_ACTIVE_LOW>,
+		   <&gpio1 10 GPIO_ACTIVE_LOW>;
 	status = "okay";
+
+	tpm@1 {
+		compatible = "tcg,tpm_tis-spi";
+		reg = <0x1>;
+		spi-max-frequency = <36000000>;
+	};
 };
 
 &gpio1 {
@@ -201,6 +208,7 @@
 			MX8MM_IOMUXC_ECSPI2_MOSI_ECSPI2_MOSI	0xd6
 			MX8MM_IOMUXC_ECSPI2_MISO_ECSPI2_MISO	0xd6
 			MX8MM_IOMUXC_ECSPI2_SS0_GPIO5_IO13	0xd6
+			MX8MM_IOMUXC_GPIO1_IO10_GPIO1_IO10	0xd6
 		>;
 	};
 
