From 63423f4f48afc96949a63c53203faa904a85670b Mon Sep 17 00:00:00 2001
From: Dave Stevenson <dave.stevenson@raspberrypi.com>
Date: Tue, 25 Feb 2020 17:35:10 +0000
Subject: [PATCH] Fixup P030 support

I got the logic wrong for enabling pixel formats, resulting in
Pi0-3 only getting a single, invalid, format (P030 SAND).

Fixes: e07ef1d drm/vc4: Add support for DRM_FORMAT_P030 to vc4 planes

Signed-off-by: Dave Stevenson <dave.stevenson@raspberrypi.com>
---
 drivers/gpu/drm/vc4/vc4_plane.c | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

--- a/drivers/gpu/drm/vc4/vc4_plane.c
+++ b/drivers/gpu/drm/vc4/vc4_plane.c
@@ -1447,7 +1447,7 @@ struct drm_plane *vc4_plane_init(struct
 		return ERR_PTR(-ENOMEM);
 
 	for (i = 0; i < ARRAY_SIZE(hvs_formats); i++) {
-		if (hvs_formats[i].hvs5_only || hvs5) {
+		if (!hvs_formats[i].hvs5_only || hvs5) {
 			formats[num_formats] = hvs_formats[i].drm;
 			num_formats++;
 		}
