From b40561fa263f3f9b06be0dd9b9e1665478d1def6 Mon Sep 17 00:00:00 2001
From: Zidan Wang <zidan.wang@freescale.com>
Date: Fri, 25 Sep 2015 14:27:00 +0800
Subject: [PATCH] MLK-11628 ASoC: fsl_sai: add initial value for is_slave_mode

After playback audio with sai<->wm8960 sound card, is_slave_mode
will be set, but it will not be cleared. So playback audio with
sai<->sii902x sound card will have no voice.

Signed-off-by: Zidan Wang <zidan.wang@freescale.com>
---
 sound/soc/fsl/fsl_sai.c | 2 ++
 1 file changed, 2 insertions(+)

--- a/sound/soc/fsl/fsl_sai.c
+++ b/sound/soc/fsl/fsl_sai.c
@@ -265,6 +265,8 @@ static int fsl_sai_set_dai_fmt_tr(struct
 		return -EINVAL;
 	}
 
+	sai->is_slave_mode = false;
+
 	/* DAI clock master masks */
 	switch (fmt & SND_SOC_DAIFMT_MASTER_MASK) {
 	case SND_SOC_DAIFMT_CBS_CFS:
