From ef2a0bd99b1549a3a4253355be247d5dff25d720 Mon Sep 17 00:00:00 2001
From: Florian Fainelli <f.fainelli@gmail.com>
Date: Thu, 30 Apr 2020 11:49:11 -0700
Subject: [PATCH] net: dsa: b53: Remove is_static argument to b53_read_op()

This argument is not used.

Signed-off-by: Florian Fainelli <f.fainelli@gmail.com>
Reviewed-by: Andrew Lunn <andrew@lunn.ch>
Signed-off-by: David S. Miller <davem@davemloft.net>
---
 drivers/net/dsa/b53/b53_common.c | 6 +++---
 1 file changed, 3 insertions(+), 3 deletions(-)

--- a/drivers/net/dsa/b53/b53_common.c
+++ b/drivers/net/dsa/b53/b53_common.c
@@ -1495,8 +1495,7 @@ static int b53_arl_rw_op(struct b53_devi
 }
 
 static int b53_arl_read(struct b53_device *dev, u64 mac,
-			u16 vid, struct b53_arl_entry *ent, u8 *idx,
-			bool is_valid)
+			u16 vid, struct b53_arl_entry *ent, u8 *idx)
 {
 	DECLARE_BITMAP(free_bins, B53_ARLTBL_MAX_BIN_ENTRIES);
 	unsigned int i;
@@ -1561,7 +1560,8 @@ static int b53_arl_op(struct b53_device
 	if (ret)
 		return ret;
 
-	ret = b53_arl_read(dev, mac, vid, &ent, &idx, is_valid);
+	ret = b53_arl_read(dev, mac, vid, &ent, &idx);
+
 	/* If this is a read, just finish now */
 	if (op)
 		return ret;
