From 23c5ff3143ce43a76eebdf60a93436de9db39a7a Mon Sep 17 00:00:00 2001
From: Robert Marko <robimarko@gmail.com>
Date: Fri, 19 Aug 2022 00:06:27 +0200
Subject: [PATCH] arm64: dts: qcom: ipq8074: correct APCS register space size

APCS DTS addition that was merged, was not supposed to get merged as it
was part of patch series that was superseded by 2 more patch series
that resolved issues with this one and greatly simplified things.

Since it already got merged, start by correcting the register space
size as APCS will not be providing regmap for PLL and it will conflict
with the standalone A53 PLL node.

Fixes: 50ed9fffec3a ("arm64: dts: qcom: ipq8074: add APCS node")
Signed-off-by: Robert Marko <robimarko@gmail.com>
Signed-off-by: Bjorn Andersson <andersson@kernel.org>
Link: https://lore.kernel.org/r/20220818220628.339366-8-robimarko@gmail.com
---
 arch/arm64/boot/dts/qcom/ipq8074.dtsi | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

--- a/arch/arm64/boot/dts/qcom/ipq8074.dtsi
+++ b/arch/arm64/boot/dts/qcom/ipq8074.dtsi
@@ -669,7 +669,7 @@
 
 		apcs_glb: mailbox@b111000 {
 			compatible = "qcom,ipq8074-apcs-apps-global";
-			reg = <0x0b111000 0x6000>;
+			reg = <0x0b111000 0x1000>;
 
 			#clock-cells = <1>;
 			#mbox-cells = <1>;
