From b1656894eef29ecd73ee239571c7ff3449bdedf2 Mon Sep 17 00:00:00 2001
From: Padmanabha Srinivasaiah <treasure4paddy@gmail.com>
Date: Thu, 30 Dec 2021 21:45:10 +0100
Subject: [PATCH] bcm2835-v4l2-isp: Add missing lock initialization

ISP device allocation is dynamic hence the locks too.
struct mutex queue_lock is not initialized which result in bug.

Fixing same by initializing it.

[   29.847138] INFO: trying to register non-static key.
[   29.847156] The code is fine but needs lockdep annotation, or maybe
[   29.847159] you didn't initialize this object before use?
[   29.847161] turning off the locking correctness validator.
[   29.847167] CPU: 1 PID: 343 Comm: v4l_id Tainted: G         C        5.15.11-rt24-v8+ #8
[   29.847187] Hardware name: Raspberry Pi 4 Model B Rev 1.4 (DT)
[   29.847194] Call trace:
[   29.847197]  dump_backtrace+0x0/0x1b8
[   29.847227]  show_stack+0x20/0x30
[   29.847240]  dump_stack_lvl+0x8c/0xb8
[   29.847254]  dump_stack+0x18/0x34
[   29.847263]  register_lock_class+0x494/0x4a0
[   29.847278]  __lock_acquire+0x80/0x1680
[   29.847289]  lock_acquire+0x214/0x3a0
[   29.847300]  mutex_lock_nested+0x70/0xc8
[   29.847312]  _vb2_fop_release+0x3c/0xa8 [videobuf2_v4l2]
[   29.847346]  vb2_fop_release+0x34/0x60 [videobuf2_v4l2]
[   29.847367]  v4l2_release+0xc8/0x108 [videodev]
[   29.847453]  __fput+0x8c/0x258
[   29.847476]  ____fput+0x18/0x28
[   29.847487]  task_work_run+0x98/0x180
[   29.847502]  do_notify_resume+0x228/0x3f8
[   29.847515]  el0_svc+0xec/0xf0
[   29.847523]  el0t_64_sync_handler+0x90/0xb8
[   29.847531]  el0t_64_sync+0x180/0x184

Signed-off-by: Padmanabha Srinivasaiah <treasure4paddy@gmail.com>
---
 drivers/staging/vc04_services/bcm2835-isp/bcm2835-v4l2-isp.c | 1 +
 1 file changed, 1 insertion(+)

--- a/drivers/staging/vc04_services/bcm2835-isp/bcm2835-v4l2-isp.c
+++ b/drivers/staging/vc04_services/bcm2835-isp/bcm2835-v4l2-isp.c
@@ -1294,6 +1294,7 @@ static int register_node(struct bcm2835_
 	int ret;
 
 	mutex_init(&node->lock);
+	mutex_init(&node->queue_lock);
 
 	node->dev = dev;
 	vfd = &node->vfd;
