From 1b9827ceab08450308f7971d6fd700ec88b6ce67 Mon Sep 17 00:00:00 2001
From: Lorenzo Bianconi <lorenzo@kernel.org>
Date: Sat, 3 Dec 2022 14:20:37 +0100
Subject: [PATCH 098/250] net: mtk_eth_soc: enable flow offload support for
 MT7986 SoC

Since Wireless Ethernet Dispatcher is now available for mt7986 in mt76,
enable hw flow support for MT7986 SoC.

Signed-off-by: Lorenzo Bianconi <lorenzo@kernel.org>
Link: https://lore.kernel.org/r/fdcaacd827938e6a8c4aa1ac2c13e46d2c08c821.1670072898.git.lorenzo@kernel.org
Signed-off-by: Jakub Kicinski <kuba@kernel.org>
---
 drivers/net/ethernet/mediatek/mtk_eth_soc.c | 1 +
 1 file changed, 1 insertion(+)

--- a/drivers/net/ethernet/mediatek/mtk_eth_soc.c
+++ b/drivers/net/ethernet/mediatek/mtk_eth_soc.c
@@ -4334,6 +4334,7 @@ static const struct mtk_soc_data mt7986_
 	.hw_features = MTK_HW_FEATURES,
 	.required_clks = MT7986_CLKS_BITMAP,
 	.required_pctl = false,
+	.offload_version = 2,
 	.hash_offset = 4,
 	.foe_entry_size = sizeof(struct mtk_foe_entry),
 	.txrx = {
