From 9ecf44fedc17ff267968b5fff589bf6793fc7ddd Mon Sep 17 00:00:00 2001
From: Jimmy Hon <honyuenkwun@gmail.com>
Date: Sun, 26 Nov 2023 14:08:45 -0600
Subject: [PATCH] arm64: dts: rockchip: add USB3 host on rk3588s-orangepi-5

Enable USB3 host controller for the Orange Pi 5.

Signed-off-by: Jimmy Hon <honyuenkwun@gmail.com>
Link: https://lore.kernel.org/r/20231126200845.1192-1-honyuenkwun@gmail.com
Signed-off-by: Heiko Stuebner <heiko@sntech.de>
---
 arch/arm64/boot/dts/rockchip/rk3588s-orangepi-5.dts | 4 ++++
 1 file changed, 4 insertions(+)

--- a/arch/arm64/boot/dts/rockchip/rk3588s-orangepi-5.dts
+++ b/arch/arm64/boot/dts/rockchip/rk3588s-orangepi-5.dts
@@ -660,3 +660,7 @@
 &usb_host1_ohci {
 	status = "okay";
 };
+
+&usb_host2_xhci {
+	status = "okay";
+};
