--- a/drivers/net/wireless/ath/ath10k/Kconfig
+++ b/drivers/net/wireless/ath/ath10k/Kconfig
@@ -86,6 +86,12 @@ config ATH10K_TRACING
 	help
 	  Select this to ath10k use tracing infrastructure.
 
+config ATH10K_THERMAL
+	bool "Atheros ath10k thermal monitoring support"
+	depends on THERMAL
+	---help---
+	  Select this to ath10k use hwmon for thermal measurement.
+
 config ATH10K_DFS_CERTIFIED
 	bool "Atheros DFS support for certified platforms"
 	depends on ATH10K && CFG80211_CERTIFICATION_ONUS
--- a/drivers/net/wireless/ath/ath10k/Makefile
+++ b/drivers/net/wireless/ath/ath10k/Makefile
@@ -18,7 +18,7 @@ ath10k_core-y += mac.o \
 ath10k_core-$(CPTCFG_ATH10K_SPECTRAL) += spectral.o
 ath10k_core-$(CPTCFG_NL80211_TESTMODE) += testmode.o
 ath10k_core-$(CPTCFG_ATH10K_TRACING) += trace.o
-ath10k_core-$(CONFIG_THERMAL) += thermal.o
+ath10k_core-$(CPTCFG_ATH10K_THERMAL) += thermal.o
 ath10k_core-$(CPTCFG_MAC80211_DEBUGFS) += debugfs_sta.o
 ath10k_core-$(CONFIG_PM) += wow.o
 ath10k_core-$(CONFIG_DEV_COREDUMP) += coredump.o
--- a/drivers/net/wireless/ath/ath10k/thermal.h
+++ b/drivers/net/wireless/ath/ath10k/thermal.h
@@ -25,7 +25,7 @@ struct ath10k_thermal {
 	int temperature;
 };
 
-#if IS_REACHABLE(CONFIG_THERMAL)
+#if IS_REACHABLE(CPTCFG_ATH10K_THERMAL)
 int ath10k_thermal_register(struct ath10k *ar);
 void ath10k_thermal_unregister(struct ath10k *ar);
 void ath10k_thermal_event_temperature(struct ath10k *ar, int temperature);
--- a/local-symbols
+++ b/local-symbols
@@ -165,6 +165,7 @@ ATH10K_SNOC=
 ATH10K_DEBUG=
 ATH10K_DEBUGFS=
 ATH10K_SPECTRAL=
+ATH10K_THERMAL=
 ATH10K_TRACING=
 ATH10K_DFS_CERTIFIED=
 WCN36XX=
