From 8d858d9c57a0210ca1ce9e5ba76fab8bdb4d7b39 Mon Sep 17 00:00:00 2001
From: Claudiu Beznea <claudiu.beznea@microchip.com>
Date: Fri, 22 Jan 2021 14:21:32 +0200
Subject: [PATCH 137/247] drivers: soc: atmel: use GENMASK

Use GENMASK() to define CIDR match mask.

Signed-off-by: Claudiu Beznea <claudiu.beznea@microchip.com>
Signed-off-by: Nicolas Ferre <nicolas.ferre@microchip.com>
Link: https://lore.kernel.org/r/1611318097-8970-3-git-send-email-claudiu.beznea@microchip.com
---
 drivers/soc/atmel/soc.c | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

--- a/drivers/soc/atmel/soc.c
+++ b/drivers/soc/atmel/soc.c
@@ -27,7 +27,7 @@
 #define AT91_CHIPID_EXID		0x04
 #define AT91_CIDR_VERSION(x)		((x) & 0x1f)
 #define AT91_CIDR_EXT			BIT(31)
-#define AT91_CIDR_MATCH_MASK		0x7fffffe0
+#define AT91_CIDR_MATCH_MASK		GENMASK(30, 5)
 
 static const struct at91_soc __initconst socs[] = {
 #ifdef CONFIG_SOC_AT91RM9200
