From 5e425e6eca155c162da58d4e58e896ed4109c7fd Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Marek=20Beh=C3=BAn?= <kabel@kernel.org>
Date: Mon, 8 Jul 2024 13:40:02 +0200
Subject: [PATCH 10/11] platform: cznic: turris-omnia-mcu: Depend on WATCHDOG
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

Add depend on WATCHDOG, otherwise modpost fails with
  ERROR: modpost: "watchdog_init_timeout" [drivers/platform/cznic/turris-omnia-mcu.ko] undefined!
  ERROR: modpost: "devm_watchdog_register_device" [drivers/platform/cznic/turris-omnia-mcu.ko] undefined!

Fixes: ab89fb5fb92c ("platform: cznic: turris-omnia-mcu: Add support for MCU watchdog")
Reported-by: kernel test robot <lkp@intel.com>
Closes: https://lore.kernel.org/oe-kbuild-all/202407040711.g19y3cWq-lkp@intel.com/
Signed-off-by: Marek Behún <kabel@kernel.org>
Link: https://lore.kernel.org/r/20240708114002.4285-3-kabel@kernel.org
Signed-off-by: Arnd Bergmann <arnd@arndb.de>
---
 drivers/platform/cznic/Kconfig | 1 +
 1 file changed, 1 insertion(+)

--- a/drivers/platform/cznic/Kconfig
+++ b/drivers/platform/cznic/Kconfig
@@ -17,6 +17,7 @@ config TURRIS_OMNIA_MCU
 	depends on MACH_ARMADA_38X || COMPILE_TEST
 	depends on I2C
 	depends on OF
+	depends on WATCHDOG
 	select GPIOLIB
 	select GPIOLIB_IRQCHIP
 	select HW_RANDOM
