From 04cd713c3834b87fcd147e4bf7b7066cfe60fffc Mon Sep 17 00:00:00 2001
From: Sebastian Kropatsch <seb-dev@mail.de>
Date: Wed, 12 Jun 2024 22:48:14 +0200
Subject: [PATCH 5/5] arm64: dts: rockchip: Enable GPU on NanoPi R6C/R6S

Enable the Mali GPU on the FriendlyElec NanoPi R6C and R6S.

Signed-off-by: Sebastian Kropatsch <seb-dev@mail.de>
---
 arch/arm64/boot/dts/rockchip/rk3588s-nanopi-r6.dtsi | 6 ++++++
 1 file changed, 6 insertions(+)

--- a/arch/arm64/boot/dts/rockchip/rk3588s-nanopi-r6.dtsi
+++ b/arch/arm64/boot/dts/rockchip/rk3588s-nanopi-r6.dtsi
@@ -207,6 +207,12 @@
 	status = "okay";
 };
 
+&gpu {
+	mali-supply = <&vdd_gpu_s0>;
+	sram-supply = <&vdd_gpu_mem_s0>;
+	status = "okay";
+};
+
 &i2c0 {
 	pinctrl-names = "default";
 	pinctrl-0 = <&i2c0m2_xfer>;
